**Highlights**

* We propose a smart street lighting system based on IPv6-enabled wireless sensor network.
* Main drawbacks of RPL protocol for P2P communication are discussed.
* GeoRank, a new routing algorithm is proposed and its scalability is compared to RPL.
* Simulations were performed on networks extracted from real street maps.
* GeoRank is adaptive to variable link densities found in large-scale networks.